Installing the NVDA Add-on for the Zoomax eReader

1. Open NVDA.
2. Press NVDA key-n to open the NVDA menu.
3. Select Tools.
4. Select Manage Add-ons.
5. Select Install.
6. Navigate to the file NLSeReaderZoomax-Driver-2023-1.nvda-addon and press Enter.
7. Tab to Yes that you are sure you want to install this add-on and Press Enter.
8. Tab to Close and press Enter.
9. Then, tab to Yes, you want to restart NVDA.
10. Connect the eReader to the computer via USB.
11. On the eReader, select Settings, the USB Mode. Alternatively, tap the On key and select USB.
12. In NVDA, press the NVDA key-n to open the NVDA menu.
13. Select Preferences, then Settings, then Braille.
14. Tab to Change and press Enter.
15. Use arrow keys to move to NLS eReader Zoomax on the list.
16. Tab to the port selection list and arrow to CH340.
17. Tab to OK.

Note: If you don’t have port ch340, install ch340ser.exe.